Project #:  	County:  	Sheet:		of		

Fabricator:  	Shop Order:  	Joint: 	

Top Flange		Bottom Flange		Tension		Compression		

Girders:  	

Material thickness:  	Material thickness:  	

Transducer Angle:  	Transducer Angle:  	

Sound Path:	Leg 1		& Leg 2		Sound Path:	Leg 1		& Leg 2		

Surface Distance:	Leg 1		& Leg 2		Surface Distance:	Leg 1		& Leg 2		

Additional Decibels:	Leg 1		& Leg 2		Additional Decibels:	Leg 1		& Leg 2		

Special Instructions:  	

	
NOTE: Use a 5” range when possible/ calculations are based on the transducer angle shown above, if angle changes pencil in new calculations.

LEG 1

LEG 2

LEG 2

FACE A

FACE B

LEG 1

LEG 1

LEG 2

LEG 2

LEG 1

FACE A	

		
FACE B

LEG 1

LEG 1